

**ELECRAFT K3 TYPE MOUNT BRACKETS**

** **

RIGHT SIDE USE

UPPER FEET HOLES

LEFT SIDE USE

HANDLE HOLES

**DRILL LEFT HANDLE HOLES & REMOVE FEET FOR RIGHT**

**STEPS TO INSTALLING YOUR 90 DEGREE “L” BRACKETS:**

* **YOU WILL NEED A THREADED NUT INSERTER KIT AND 8/32 SIZE RIVET-NUTS**
* **NOVEXCOMM CAN PROVIDE THEM BUT THEY ARE AVAILABLE ELSEWHERE**
* **WE ALSO OFFER A SIMPLE ONE-RADIO KIT OF A GRADE-8 BOLT & WRENCH**
* **REMOVE THE TOP COVER AND VIEW THE SPACES LEFT & RIGHT**
* **YOU DO NOT NEED TO UNSCREW THE LEFT OR RIGHT SIDES!**
* **REMOVE THE HANDLES ON THE LEFT SIDE AND CAPTURE THE LOOSE NUTS**
* **TURN THE OPEN TOP RADIO UPSIDE DOWN TO LET DRILL SHAVINGS FALL**
* **DRILL THE TWO HOLES OUT TO FIT RIV-NUTS;(¼” OR 15/64 SIZE BIT)**
* **PRY OUT 4 RUBBER FEET FROM THE RIGHT SIDE & INSTALL RIV-NUTS *HIGH***
* **INSERT AND SET THE NEW THREADED INSERTS IN EACH SIDE, REASSEMBLE**
* **USE THE WASHERS ON EACH BOLT TO PREVENT LONG SCREW PENETRATION**
* **POSITION THE “L” BRACKETS ON THE TRAY WHERE YOU WANT THE RADIO**
* **MARK AND DRILL THE TRAY FOR THE 4 BRACKETS, BOLT THEM LOOSELY**
* **THEN FINAL-TIGHTEN ALL 4 OF THE BRACKETS TO STABILIZE THE RADIO**

***STILL HAVE QUESTIONS? CALL OUR WILDLY BRILLIANT TECHNICANS*!**

[**www.Novexcomm.com**](http://www.Novexcomm.com) **310.534.4456 M-F 10-6 Pacific (California) time**

**Call or email if you want us to provide either the tool or the “one-radio” kit.**